*****************************************************************

Cas Studio 9.8.3 - RELEASE INFORMATION - PLEASE READ CAREFULLY

*****************************************************************
SETUP

If this is the first time you install the software, remember to run the setup the device NOT connected!

Once you installed the software launch it and follow the screen instructions.
When Windows asks for drivers, direct it into the folder where you installed the software previously.

(ex. c:\program files\duolabs\cas interfacxe studio ...\drivers as default)

or to the DRIVER folder inside the zip where you found this file

If you have problems with driver :

- Check in your Control Panel -> System -> Hardware Tab -> Device Manager.
- Check if you see USB Device in the list, or inside the USB Hub tab.
- If you see a yellow mark on USB Device , right click on the USB Device and click on update Driver.
- Let windows search for your driver in the DRIVER folder that you find in the zip file.
- Follow windows to have the drivers installed.

For other problem please press the help button in the software before sending your question to support@duolabs.com

Versione 9.8.6:

- Bug Fixed for DIABLO GSM.
- Minor Bug Fixed.

Versione 9.8.5:

- Added support for AlphaCrypt Light Cam.
- Minor Bug Fixed.

Versione 9.8.4:

- Bug Fixed for DIABLO GSM.
- Minor Bug Fixed.

Versione 9.8.3:

- Bug Fixed for DIABLO LAN and DIABLO WIFI.
- Minor Bug Fixed.

Versione 9.8.2:

- Added support for DIABLO LAN.
- Minor Bug Fixed.

Versione 9.8.1:

- Added support for DIABLO GSM.
- Minor Bug Fixed.

Versione 9.8.0:

- Bug Fixed for DiabloLight TO Diablo2 update.
- Minor Bug Fixed.

Versione 9.7.1:

- Minor Bug Fixed.

Versione 9.7.0:

- Minor Bug Fixed.

Versione 9.6.0:

- Added support for DIABLO WIFI HW Rev2.6.
- Minor Bug Fixed.

Versione 9.5.0:

- Added support for DIABLO2PRO.
- Minor Bug Fixed.

Versione 9.4.0:

- Added support for DIABLO2 lite TWIN.
- Minor Bug Fixed.

Versione 9.3.0:

- Minor Bug Fixed.

Versione 9.2.0:

- Added support for new cam VU+.
- Bug Fix DIABLO2 rev. HW 4.0 backup/restore functions.
- Minor Bug Fixed.

Versione 9.1.0:

- Fix bug with update function from Diablo Lite 2.2/2.3 to Diablo 2 HW. 4.0 with Vista/Windows 7.
- Minor Bug Fixed.

Versione 9.0.1:

- Added support for Jolly CAM.
- Added Update Diablo Lite 2.2/2.3 To Diablo 2 HW 4.0.
- Minor Bug Fixed.

Versione 9.0.0:

- Added support for Diablo2 HW 4.0.
- Bug Fix in CAM Explorer for CAS2 PLUS.
- Bug Fix for GIGA CAM for CAS3.
- Minor Bug Fixed.

Versione 8.8.0:

- Added support for Diablo WiFi HW rev. 2.4.
- Minor Bug Fixed.

Versione 8.7.1:

- Minor Bug Fixed.

Versione 8.7:

- DiABLO 2 LITE. Added DIABLO2 LITE.

Versione 8.6c:

- GAMMA Card. Added Erase and program with .GAM file

Versione 8.6b:

- Problemi di programmazione delle Diablo con alcuni CAS Interface 2 Plus risolti
- Update 2.2 cam to 2.3 added inside cas studio
- Dragon 99% error solved
- Problem updating diablo with cas2 solved
- Format/Fdisk problems solved

Versione 8.5b:

- Editing of WiFi configuration of WiFi Diablo Cam.

Versione 8.5:

- Suppport for WiFi Diablo Cam.

Versione 8.4:

- Fixed some bugs with Cas Interface 2

Versione 8.3a:

- Bug on Erasing cams in some cas3 plus solved

Versione 8.3:

- Minor bug solved

Versione 8.2:

- GigaCam programming added
- Drivers problems with windows98 and some setup problems solved
- SIM reading problem solved on some card type

Versione 7.9c:

- Support for the new Dynamite Plus added
- Bug found in some Reborn on erase function

Versione 7.9b:

- Bug in dragon programming fixed ( found in 7.9a )

Versione 7.9a:

- Bug in matrix programming fixed

Versione 7.9:

- Anaconda programming added.
- Sistemata la programmazione della cam Dragon 2.05 e 2.05 on Cas2 plus and Cas3 plus.
- Backup of Diablo Cam added.
- Rename of files inside the Diablo file system added.
- refer to www.diablocam.com for new firmware and software for Diablo cams

Release 7.8:

- This new release supports the new version of Cas Interface 2 Plus
- New way of dragon cam programming
  - Now you can insert your dummy card in the cam, go in the dragon cam programming module, choose the file and put the cam in the receiver.
    In way we should solve some problems that happens on some pc or in some cam.

Release 7.7:

- Super Dragon programming added.

Release 7.6:

- Support for CAS Interface 3 Plus for all functions added.

Release 7.5:

- Bug with Funcard fixed ( Runtime error 35600 ).
- Problems reading some phone sim card fixed.
- K3 programming added( Cas3, Cas2+addon, Dynamite, Dynamite Plus ).
- Diablo programming problem Fixed.

Release 7.4 :

- Xcam Cam repairing problems fixed.
- Xcam Premium ( not the orion one ) added.
- DIDEM programming with Dynamite Plus added.
- Dragon Cam repairing problems fixed.
- Daytona card programming added for Dynamite Plus
- File copying to Diablo cam fixed ( the problem was in windows configured with file extension hidden )

Release 7.3 :

- SimEditor updated to support H3G Sim Cards
- Diablo CAM Light and Wireless can now be programmed with Cas Interface 2 ( only cams with firmware starting from 1.3 )

Release 7.2 :

- Support for the new Cas Interface 3 boards

Release 7.1 :

- Fixed DiabloCam programming minor bug.
- Fixed Dragon Cam 2.xx programming bug with Cas Interface 3.
- Added Daytona smartcard programming.

Release 7.0a :

- Added DIABLOCAM Wireless and DIABLOCAM LIGHT programming with CAS Interface 3 and CAS Interface 2 Plus!
- Added DIDEM Card programming.
- Fixed driver installation with Windows Server 2003
- Fixed minor bugs.

Release 6.9 :

- Bugs solved with ATMEGA , FUN CARD and PIC programming.

Release 6.8 :

- Cerebro card programming added

Release 6.7 :

- new CAS Interface 2 PLUS supported.
- Some problems with XCAM,Dragon,Matrix
- T-REX added

Release 6.6 :

- Fixed some problem with many cams
- added T-REX cam button

Release 6.6 :

- CAS Interface 2 PLUS is now supported

Release 6.5 :

- XCAM and DRAGON updating problem on some pc solved
- XTREME programming with addon module did not appear

Release 6.4 :

- XCAM updating problem on some pc solved

CARD GENERATOR is now available also for ADDON and DYNAMITE

Release 6.3 :
What's new in 6.3?

The new funcion Smartcard -> Card Generator!

It will be now possible to erase the exisiting OS on your M2/Platinum Card and load a new different OS (like OPOS 1.03 or Titanium2). We are actually working to implement the erasing of other OS Card.
Once the card is erased you are ready to load the new OS and you need to know the Transport Code. Cas Studio will set a Transport Code as default which is the most used one but this doens't mean your OS Card has that Transport Code.All you do you do it at your own risk!
If you don't know what you are doing simply don't do it! You could permanently damage your card! You have been told! Don't upload files you don't know what they are anyway!

How to use the Card Generator?

Do you have a virgin AT90SC6464C?

It will be enought that you insert the Smartcard into the Card reader of the Cas Interface 3.
On the Card Info you will see the following information:

Status-memory State: 90 00 = Blank card
BootLoader Version: XX XX
Chip Identifier: AT90SC6464C

This means that your Smartcard is blank and ready to be programmed.

- Press "Open File" and choose the file you want to load with the extension .OSF
  You sohuld see a short description of the kind of file you are loading if available.
- Now press the button "Write" to proceed with the OS loading into the card.
  At the end of this procedure the ATR will be performed.

Is your Smartcard is not blank (pre-programmed) as OS Card?

You have to make sure it's a M2 or Platinum card. Insert the Smartcard into the card reader and the funcion "Erase" will be enabled.
At this point you can press the "Erase" button. Make sure you have the valid Trasport Code otherwise your Smartcard would not be accessible anymore!
Wait util the Smartcard is erased and the new ATR will come up as shown:

Status-memory State: 90 03 = Pre-Programmed Card
BootLoader Version: XX XX
Chip Identifier: AT90SC6464C

This means that your Smartcard is blank and ready to be programmed.

- Press "Open File" and choose the file you want to load with the extension .OSF
  You sohuld see a short description of the kind of file you are loading if available.
- Now press the button "Write" to proceed with the OS loading into the card.
  At the end of this procedure the ATR will be performed.

About the Transport Code:

The Transport Code works almost in the same way as the PIN function of your GSM Sim-Card. You need it to access to all the functions of a Blank or erased Smartcard.
Just before programming a blank or Erased Smartcard you will need to present the Trasport Code. If you present the Trasport Code for more than 3 times wrong the card will be permanently blocked and there will be no more possibilities to access to the card anymore!
Set as default there is a Trasport Code which is quite standard. This doens't mean it the correct Trasport Code for your Card. Don't erase neither try to program a blank or erased Smartcard if you are not sure about the genuinity of your Transport Code.

And now .... Enjoy!

Problem with DRAGON CAM programming fixed .

Button HELP added to every form, it link to a internet page that will be updated in the future, in this way you can have a updated manual.

Release 6.2 :

- Problem with Matrix revolution with "00000000" solved for CAS3
- Option to read the ram of the cam when it's working ( only for experts )
- Working with key editing in the Host Module fixed
- Joker cam supported by the Host Module
- Neotion added in the cam list
- Titan 2 added in the card list
- XCAM programming simplified ( now you only need to choose the file )
- Some languages added: Arabian, Slovak, Croatian, Norvegian.
- Dragon 2.05 is now supprted ( we suppose 2.06 is working )
- Fixed some bugs in Host Module.
- Problem with ATHLON processor fixed.

Release 6.1 :

- Now CIS support XCAM orion based
- XCAM 1.3 and 1.4 can be now repaired
- Fixed SIM Card problems
- Fixed minor bugs
- More languages added ( thanks to the the people who help us in translation )
- Aggiunta la programmazione della WILD CARD