Upgrade Spark by USB

1. Make sure [C:/spark] is exist, if not, please create this folder.
2. copy [mImage] and [userfsub.img] to [C:/spark]
3. Connect USB stick to STB
4. Keep Pressing [OK] Button in Front Panel, then power on STB.
5. After 5 seconds, you will see [Forc] in LED, release [OK] button and press [Right] Button.
6. if everything OK, You will see [U LD] shining in LED
7. if upgrade success, You will see [SUCC] and STB reboot automatically
8. If upgrade not finishes in 5 minutes, then there must be something wrong, please check
your configuration and re-try.

_____________________________________________________________________________________________

Upgrade Spark by TFTP

1. copy [mImage] and [userfsub.img] to any folder of your PC, for example [C:/spark]
2. select folder in TFTP tools
3. Keep Pressing [OK] Button in Front Panel, then power on STB.
4. After 5 seconds you will see [Forc] in LED, release [OK] button and press [Right] Button.
5. if everything OK, You will see [T LD] shining in LED and you will see some debug
information in TFTP Server, like
“ Mon Oct 25 14:02:36 2010: Sending 'mImage' file to 192.168.40.19 in binary mode
Mon Oct 25 14:02:39 2010: Successful.
Mon Oct 25 14:02:50 2010: Sending 'userfsub.img' file to 192.168.40.19 in binary mode
Mon Oct 25 14:03:33 2010: Successful.”
6. if upgrade success, You will see [SUCC] and STB reboot automatically


     


     GREETZ FROM 
E.O.S. Developer Team
       LG TBX 